**Configuración switch:**

**Crear vlan:**

# vlan “x”

# name “x”

**Configurar int:**

# Int “fax/x” o int range “fax/x-x”

# switchport mode access

# switch access vlan “x”

**Configurar trunking:**

# Int “fax/x” o int range “fax/x-x”

# switchport mode trunk

# switchport nonegotiate

# switchport trunk native vlan “x”

# switchport native vlan “x” (router)

**Configurar router:**

# int “fax/x.x”

# encapsulation dot1Q “x”

# ip address “Puerta de enlace” “Máscara”

# no shutdown

# int “fax/x”

# no shutdown